How to ask for current power state (1=On, 0=Standby) for all device attached to a computer network interface (NIC) 169.254.1.112 using the dynamic port option:

>paraDlm.exe 169.254.1.112 -dynamic "Dev.Power?"

Hint: This also gives you all the Frame IDs which you can use to address a specific device.

______________________
How to set power state (1=On, 0=Standby) for one device (Frame ID=3d000011:d6ed9201) on computer network interface (NIC) 169.254.1.112 using the dynamic port option:

>paraDlm.exe 169.254.1.112 -dynamic 3d000011:d6ed9201 "Dev.Power=1"

______________________
How to, for Module A, set Module Input mute (1=Mute, 0=Unmute) for all devices on the network using dynamic port. 

>paraDlmx.exe 169.254.1.112 -dynamic "Mod.In.Mute=A 1"

_______________________
How to, for Power channel 4 (Power output D) set Amp channel mute (1=Mute, 0=Unmute) for all device on the network using dynamic port: 

>paraDlm.exe 169.254.1.112 -dynamic "Dev.Pwr.Mute=4 1"
