This is an example on how to ask for power state (1=On, 0=Standby) for one device (Frame ID=3d000011:d6ed9201) on computer network interface (NIC) 10.10.10.116:
>dlmTestLite 10.10.10.116 3d000011:d6ed9201 "Dev.Power?"